## Input
RB Series Earlier Models

SuperLab provides support for all the legacy RB Series response pads. These are:

RB-420 RB-410 RB-400
RB-620 RB-610 RB-600
RB-520
RB-820

Click on the Setup tab to change the model and select the serial port. SuperLab will show all the serial ports that are available on your computer.

SuperLab automatically creates a number of responses based on the selected model. You can edit or delete them. A response can consist of a key press or a key release. If you need a response that consists of a key release, make sure that the Ignore the key release checkbox in the Options tab is turned off. It is a good idea to give the response a descriptive name, e.g. “target” or “same”.

### Available Options

The following options are available for the RB Series Earlier Model Pad input device:

- Ignore the key release: If your experiment needs a response that consists of a key release, this option should be turned off. Otherwise it is a good idea to keep this option turned on.

- Wait until the key is released: When this option is turned on, SuperLab will not advance to the next event or the next trial (depending on which sub-option is selected) until the participant has released the response pad key.